This CD-ROM answer product uses Schlumberger corporate standard formats for delivery of all processing results. Helper applications are available for most of these formats on most operating systems. If your browser has been configured to take advantage of these helper applications, you should be able to access processing results directly from your browser. Reports are supplied in PDF format. PDF is a portable document format developed by Adobe, and can be viewed using the freeware Adobe Acrobat Reader. Acrobat Reader 5.0 for use with Microsoft Windows can be installed from this CD-ROM. Acrobat Reader software for most other common operating systems is available for download from Adobe's web site. We recommend using Acrobat Reader version 4.0 or higher. Log graphics are supplied in PDS format. Other graphics formats include CGM, TIFF and PDF. PDS is an image format designed by Schlumberger specifically for log graphics. It is a graphics metafile format used to efficiently describe, store, and transport log graphics. PDSView 3.0, a software product for use with Microsoft Windows which allows for viewing and printing of pds files, as well as conversion of PDS files to CGM and GIF formats, can be installed from this CD-ROM. BlueView is a software application which allows for displaying, annotating, editing, splicing and printing of images on a Windows system. With the BlueView application, Schlumberger PDS files can be converted and saved as TIFF files. Images can be saved to any common raster format at any color depth and in several types of compressed file formats. The transparency function of the BlueView application can be used to make overlay images for a full and quick comparison. BlueView can also be installed from this CD-ROM. Digital log data is supplied in either DLIS or LAS format. DLIS is an industry standard file format for well log data as defined by Recommended Practice 66 of the American Petroleum Institute. LAS is a standard published by the Canadian Well Logging Society of ASCII data. The Schlumberger Log Data Toolbox 2.2, a Microsoft Windows based set of utility programs for manipulating digital log data, can be installed from this CD-ROM. The Log Data Toolbox includes DLIS to ASCII and DLIS to LIS converters, and DLIS and ASCII verification tools. Seismic data is supplied in SEGY format. SEGY is an industry standard file format for seismic data as defined by the SEG. Verification listings in text format are included. Spreadsheet data is generally supplied in Microsoft EXCEL format or Adobe PDF format. For more information on these Schlumberger software applications, please use the link to the Schlumberger Connect website above or contact your local Schlumberger representative, or one of the Data Services Centres listed below. Schlumberger - Data and Consulting Services Level 5, 256 St Georges Terrace, Perth WA 6000 Australia Telephone +61 8 94204800 Facsimile +61 8 94204715 E-mail dcs@perth.oilfield.slb.com