Verification listing of 'Y4_synt_R35.sgy'
----------------------------------------------------------------------------
File 1 :
--------



Record 1 :
----------
  Offset : 1
  Size : 3200 bytes



EBCDIC header (record 1) :
--------------------------
  Offset : 1
  Size : 3200 bytes
  Format : EBCDIC

C1 CLIENT: ORIGIN ENERGY CONTRACTOR: SCHLUMBERGER SURVEY DATE: 15-JUL-2004      
C2 COUNTRY: AUSTRALIA   WELL NAME:   YOLLA-4                                    
C3 VSP SURVEY DESCRIPTION: OFFSHORE BOAT SOURCE VIVSP                           
C4 TAPE FORMAT:  SEGY   MEASUREMENT SYSTEM: M                                   
C5 WELL COORD: LON: 145 49' 06.0569"E LAT: 39 50' 40.5920"S                     
C6 SRD: MEAN SEA LEVEL  VSP LOG DATUM: KB     KB : 43M  GL: -81M                
C7 WELL DEVIATION: MAX 25.6 DEG                                                 
C8 SOURCE: AIRGUN AT VERTICAL INCIDENCE / -6M / REF -9.2M                       
C9 DOWNHOLE SENSOR TYPE: 3C ACCELEROMETER (VSI-4)                               
C10                                                                             
C11 DESCRIPTION: SYNTHETIC SEISMOGRAM RICKER 35 Hz                              
C12                                                                             
C13 PROCESSING HISTORY:                                                         
C14 (0) Load Data                                                               
C15 (1) Edit Bad Records                                                        
C16 (2) Pick Reference Break                                                    
C17 (3) Z Component Median Stack                                                
C18 (4) Geophone Transform                                                      
C19 (5) Pick Break Time                                                         
C20 (6) Survey Geometry + SRD Correction                                        
C21 (7) Bandpass Filter 5-95 Hz                                                 
C22 (8) Rotation to V and H components                                          
C23 (9) Signature Deconvolution: PDN, Gap 55 ms, Window 0.85s                   
C24 (10) Geometrical Spreading Correction: Exponent 1.56                        
C25 (11) RMS Normalization: Window 200 ms                                       
C26 (12) Wavefield Separation:  Velocity Filters 11x1 Tri Mean                  
C27 (13) Waveshaping Deconvolution:  5/60 Hz Zero Phase  / 0.5s                 
C28 (14) Upgoing Enhancement: Velocity Filter 7x3 Tri Mean                      
C29 (15) Shift to Two Way Time                                                  
C30 (16) Corridor Stack: 100 ms Window + Deepest 8 Traces                       
C31 (17) Sonic Editing                                                          
C32 (18) Sonic Calibration with VSP data                                        
C33 (19) Synthetic Seismogram Generation : Zero Phase Ricker 35 Hz              
C34                                                                             
C35                                                                             
C36                                                                             
C37                                                                             
C38                                                                             
C39                                                                             
C40 END EBCDIC                                                                  







Record 2 :
----------
  Offset : 3201
  Size : 400 bytes



BINARY header (record 2) :
--------------------------
  Offset : 1
  Size : 400 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 24

JOBID                                    :   1 -   4 : 0
LINE_NUMBER                              :   5 -   8 : -999
ACQUISITION_FILE_NUMBER                  :   9 -  12 : -999
NBR_DATA_TRACE                           :  13 -  14 : 1
NBR_AUX_TRACE                            :  15 -  16 : 0
SAMPLING_PERIOD                          :  17 -  18 : [ us ] 1000
ORIGINAL_SAMPLING_PERIOD                 :  19 -  20 : [ ms ] 0
NSAMPLES                                 :  21 -  22 : 2243
ORIGINAL_NSAMPLES                        :  23 -  24 : 0
DATA_CODE                                :  25 -  26 : 1
VERTICAL_SUM_CODE                        :  31 -  32 : 0
SWESF                                    :  33 -  34 : [ Hz ] 0
SWEEF                                    :  35 -  36 : [ Hz ] 0
SWEEL                                    :  37 -  38 : [ ms ] 0
SWETYP                                   :  39 -  40 : 0
SWEEP_TRACEID                            :  41 -  42 : 0
TAPSL                                    :  43 -  44 : [ ms ] 0
TAPEL                                    :  45 -  46 : [ ms ] 0
TAPTYP                                   :  47 -  48 : 0
CORRELATED                               :  49 -  50 : 0
BINARY_GAIN_RECOVERY                     :  51 -  52 : 0
AMPL_RECOVERY_METHOD                     :  53 -  54 : 0
MEASUREMENT_SYSTEM                       :  55 -  56 : 1
ISP                                      :  57 -  58 : 0






Record 3 :
----------
  Offset : 3601
  Size : 9212 bytes



TRACE HEADER header (record 3) :
--------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 0
TRACE_SEQ_REEL                           :   5 -   8 : 1
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 3) :
--------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 3) :
--------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 4 :
----------
  Offset : 12813
  Size : 9212 bytes



TRACE HEADER header (record 4) :
--------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 1
TRACE_SEQ_REEL                           :   5 -   8 : 2
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 4) :
--------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 4) :
--------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 5 :
----------
  Offset : 22025
  Size : 9212 bytes



TRACE HEADER header (record 5) :
--------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 2
TRACE_SEQ_REEL                           :   5 -   8 : 3
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 5) :
--------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 5) :
--------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 6 :
----------
  Offset : 31237
  Size : 9212 bytes



TRACE HEADER header (record 6) :
--------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 3
TRACE_SEQ_REEL                           :   5 -   8 : 4
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 6) :
--------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 6) :
--------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 7 :
----------
  Offset : 40449
  Size : 9212 bytes



TRACE HEADER header (record 7) :
--------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 4
TRACE_SEQ_REEL                           :   5 -   8 : 5
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 7) :
--------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 7) :
--------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 8 :
----------
  Offset : 49661
  Size : 9212 bytes



TRACE HEADER header (record 8) :
--------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 5
TRACE_SEQ_REEL                           :   5 -   8 : 6
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 8) :
--------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 8) :
--------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 9 :
----------
  Offset : 58873
  Size : 9212 bytes



TRACE HEADER header (record 9) :
--------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 6
TRACE_SEQ_REEL                           :   5 -   8 : 7
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 9) :
--------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 9) :
--------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 10 :
-----------
  Offset : 68085
  Size : 9212 bytes



TRACE HEADER header (record 10) :
---------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 7
TRACE_SEQ_REEL                           :   5 -   8 : 8
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 10) :
---------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 10) :
---------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 11 :
-----------
  Offset : 77297
  Size : 9212 bytes



TRACE HEADER header (record 11) :
---------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 8
TRACE_SEQ_REEL                           :   5 -   8 : 9
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 11) :
---------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 11) :
---------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.






Record 12 :
-----------
  Offset : 86509
  Size : 9212 bytes



TRACE HEADER header (record 12) :
---------------------------------
  Offset : 1
  Size : 240 bytes
  Format : Integer (2 & 4 bytes)
  Number of fields : 64

CLUSTER_NAME                             : not on tape: ASCII : 
LEVEL_NUMBER                             : not on tape: 
TRACE_SEQ_LINE                           :   1 -   4 : 9
TRACE_SEQ_REEL                           :   5 -   8 : 10
ACQUISITION_SHOT_NUMBER                  :   9 -  12 : -999
TRACE_SEQ_RECORD                         :  13 -  16 : 0
FRAME_NUMBER                             :  17 -  20 : -999
COMMON_DEPTHPOINT_NUMBER                 :  21 -  24 : -999
DATA_IDENTIFICATION                      :  29 -  30 : 1
SUMMED_TRACES_NUMBER                     :  31 -  32 : 0
DATA_USE                                 :  35 -  36 : 0
SOURCE_LINE_POSITION_RHO * 1             :  37 -  40 : [ m ] -999.000000
CABLE_LENGTH * 1                         :  41 -  44 : [ m ] 0.000000
SOURCE_POSITION_Z * 1                    :  49 -  52 : [ m ] 0.000000
RECEIVER_POSITION_Z * 1                  :  53 -  56 : [ m ] 0.000000
DEPTH_COEFF                              :  69 -  70 : 1
COORD_COEFF                              :  71 -  72 : 1
SOURCE_POSITION_X * 1                    :  73 -  76 : [ m ] 0.000000
SOURCE_POSITION_Y * 1                    :  77 -  80 : [ m ] 0.000000
RECEIVER_POSITION_X * 1                  :  81 -  84 : [ m ] 0.000000
RECEIVER_POSITION_Y * 1                  :  85 -  88 : [ m ] 0.000000
COORD_UNIT                               :  89 -  90 : 0
SOURCE_STATIC                            :  99 - 100 : 0
GROUP_STATIC                             : 101 - 102 : 0
TOTAL_STATIC                             : 103 - 104 : 0
TRANSIT_TIME                             : 107 - 108 : [ ms ] 0
TIME_OF_FIRST_DATA                       : 109 - 110 : [ ms ] 0
NSAMPLES                                 : 115 - 116 : 2243
SAMPLING_PERIOD                          : 117 - 118 : [ us ] 1000
GAIN_TYPE                                : 119 - 120 : [ ms ] 0
CORRELATED                               : 125 - 126 : [ ms ] 0
SWESF                                    : 127 - 128 : [ Hz ] 0
SWEEF                                    : 129 - 130 : [ Hz ] 0
SWEEL                                    : 131 - 132 : [ ms ] 0
SWETYP                                   : 133 - 134 : 0
TAPSL                                    : 135 - 136 : [ ms ] 0
TAPEL                                    : 137 - 138 : [ ms ] 0
TAPTYP                                   : 139 - 140 : [ ms ] 0
AFFREQ                                   : 141 - 142 : 0
AFSLOP                                   : 143 - 144 : 0
NFFREQ                                   : 145 - 146 : 0
NFSLOP                                   : 147 - 148 : 0
LCFREQ                                   : 149 - 150 : 0
HCFREQ                                   : 151 - 152 : 0
LCSLOP                                   : 153 - 154 : 0
HCSLOP                                   : 155 - 156 : 0
SHOT_YEAR                                : 157 - 158 : 2037
SHOT_DAY                                 : 159 - 160 : 286
SHOT_HOUR                                : 161 - 162 : 9
SHOT_MINUTE                              : 163 - 164 : 3
SHOT_SECOND                              : 165 - 166 : 59
TOOL_NUMBER                              : 175 - 176 : 0
USER_KEY_1                               : 181 - 182 : 0
USER_KEY_2                               : 183 - 184 : 0
USER_KEY_3                               : 185 - 186 : 0
USER_KEY_4                               : 187 - 188 : 0
USER_KEY_5                               : 189 - 190 : 0
USER_KEY_6                               : 191 - 192 : 0
USER_KEY_7                               : 193 - 194 : 0
USER_KEY_8                               : 195 - 196 : 0
USER_KEY_9                               : 197 - 198 : 0
USER_KEY_10                              : 199 - 200 : 0
ACQUISITION_BREAK_TIME                   : 235 - 236 : [ ms ] 0
SHAKER_CODE                              : 237 - 238 : 0





TRACE [trace] (record 12) :
---------------------------
  Offset : 241
  Size : 8972 bytes
  Format : IBM floating point (4 bytes)





TRACE FOOTER header (record 12) :
---------------------------------
  Offset : 9213
  Size : 0 bytes
  Format : Integer (2 & 4 bytes)
  No field.




