Schlumberger Verification Listing | Listing Created: 17-SEP-2009 10:48:00 Version: 11C0-208

Input Source: SpikeyBeach1_LWD_RM_RUN1.dlis Format: DLIS Storage Set ID: Default Storage Set | Max Record Length: 8192 Storage Unit Sequence: 1

File Header | File: arc_and_sonic_DLIS_Run1__16Sep09_200537__16Sep09_201655 | Sequence: 1 |
Defining Origin: 76

| File ID: arc_and_sonic_DLIS_Run1__16Sep09_200537__16Sep09_201655 | File Type: CUSTOMER |  |

| Producer Name: Schlumberger | Product/Version: HZ-OP:DnM 1.2.8706.0 | File Set: 272459720 | File Number: 1 | 16-SEP-2009 20:17:11

Company Name: | Beach Petroleum Ltd
Well Name: | Spikey Beach-1
Field Name: | Exploration
Tool String: | DRILLING_SURFACE, ARC9A-AA, MWD_10, SWD9-BA
Computations: | SURVEY, ARC9PRESSURECOMPUTATION, ARC9GAMMARAYCOMPUTATION, ARCRESISTIVITY, WAVEFORMVIEWERENSEMBLE_DNM

Well Site Data | File: arc_and_sonic_DLIS_Run1__16Sep09_200537__16Sep09_201655 | Sequence: 1 |
Origin: 76 Well Data
| Company Name | Beach Petroleum Ltd |  | CN
| Well Name | Spikey Beach-1 |  | WN
| Field Name | Exploration |  | FN
| County: | Australia |  | CLAB, COUN
| State: | Tasmania |  | SLAB, STAT
| Nation | Australia |  | NATI
| Continent | Australasia |  | CONT
| Field Location | Exploration |  | FL
| Service Order Number | 09ASQ0029 |  | SON
| Longitude | 145° 52' 24.71" E |  | LONG
| Latitude | 40° 28' 53.9" S |  | LATI
| Maximum Hole Deviation | 0.380 (deg) |  | MHD
| Elevation of Ground Level Above Permanent Datum | -74.0 (m) |  | EGL
| Elevation of Derrick Floor Above Permanent Datum | 21.5 (m) |  | EDF
| Permanent Datum | MSL | Elevation of Permanent Datum (PDAT) above Mean Sea Level 0.0 (m) | PDAT, EPD
| Logging Measured From (Name of Logging Elevation Reference) | DF | Elevation of Depth Reference (LMF) Above Permanent Datum 21.5 (m) | LMF, APD
| Drilling Measured From (Name of Drilling Elevation Reference) | DF |  | DMF
Absent Valued Parameters: CN1, FL1, FL2, SECT, TOWN, RANG, APIN, EKB Job Data
| Date of Operation | 07-Sep-2009 |  | DATE
| Run Number | 1 |  | RUN
| Total Depth (Driller) | 817.0 (m) |  | TDD
| Total Depth (Logger) | 817.0 (m) |  | TDL
| Bottom Log Interval | -999.3 (m) |  | BLI
| Top Log Interval | -999.3 (m) |  | TLI
| Casing Outer Diameter | 13.4 (in) |  | CSIZ
| Casing Depth From | 150.0 (m) |  | CDF
| Casing Shoe Depth (bottom) | 816.0 (m) |  | CADT
| Casing Grade | H50 |  | CASG
| Casing Weight | 169.6 (kg/m) |  | CWEI
| Bit Size | 17.5 (in) |  | BS
| Bit Size Depth From (Top) | 150.0 (m) |  | BSDF
| Bit Size Depth To (Bottom) | 817.0 (m) |  | BSDT
| Engineer s Name | Marganda Sihite |  | ENGI
| Witness s Name | Fred/Peter |  | WITN
| Service Order Number | 09ASQ0029 |  | SON
Absent Valued Parameters: DLAB, TLAB, LUN, LUL Mud Data
| Drilling Fluid Type | Sea Water |  | DFT
| Drilling Fluid Density | 8.80 (lbm/gal) | Drilling Fluid Viscosity 100.0 (s) | DFD, DFV
| Drilling Fluid pH | 9.00 |  | DFPH
| Fluid Interval Transit Time | 206.0 (us/ft) |  | FVEL
| Borehole Salinity | 39794.5 (ppm) |  | BSAL
| Mud Sample Source | Active Tank |  | MSS
| Resistivity of Mud Sample | 0.200 (ohm.m) | Mud Sample Temperature 15.0 (degC) | RMS, MST
| Resistivity of Mud Filtrate Sample | 0.150 (ohm.m) | Mud Filtrate Sample Temperature 20.0 (degC) | RMFS, MFST
| Mudcake Sample Temperature | 20.0 (degC) |  | MCST
| Resistivity of Mud at Bottom Hole Temperature | 0.160 (ohm.m) |  | RMB
| Resistivity of Mud Filtrate At Bottom Hole Temperature | 0.137 (ohm.m) |  | RMFB
Absent Valued Parameters: DFL, RMCS, MRT, DCS, TCS, DLAB, TLAB PVT Data
| Borehole Salinity | 39794.5 (ppm) |  | BSAL
Absent Valued Parameters: ODEN, BO, BW, IBG, BPP, BPT, SGOR Cement Data Absent Valued Parameters: CASN

Channels | File: arc_and_sonic_DLIS_Run1__16Sep09_200537__16Sep09_201655 | Sequence: 1 |
Origin: 76 DRILLING_SURFACE: DRILLING_SURFACE Spacing: 6.0 in Number of Channels: 2
| BHD ROP5
ARC9A-AA: Array Resistivity Compensated 900 Spacing: 6.0 in Number of Channels: 3
| GR_ARC GR_ARC_FILT GR_ARC_RAW
SWD9-BA: sonicVISION 900 Spacing: 6.0 in Number of Channels: 63
| AMPO AMPR1 AMPR2 AMPR3 AMPR4 ANR1 ANR2 ANR3 ANR4 ANT1 ANT2 ANT3 ANT4 C1RA C1TA CHPO CHRA CHRS CHTA CHTS DMXM DRMS DTBC DTPO DTRA DTRS DTSH DTTA DTTS ITTI MNS3 MNS4 MNSH MNSL MXS3 MXS4 MXSH MXSL N10V NPRA NPTA NWRA NWTA S1RA S1TA SPOR STRA STTA T1RA T1TA TTPO TTRA TTRS TTTA TTTS WF1G WF1I WF2G WF2I WF3G WF3I WF4G WF4I
Spacing: 1.2 in Number of Channels: 1
| TICKS_SON
Spacing: 2.0 in Number of Channels: 4
| WF1T WF2T WF3T WF4T
SURVEY: DnMSurveyEnsemble Spacing: 6.0 in Number of Channels: 2
| DEVI MD
System and Miscellaneous Spacing: 6.0 in Number of Channels: 1
| TDEP
Spacing: 1.2 in Number of Channels: 1
| TDEP;1
Spacing: 2.0 in Number of Channels: 1
| TDEP;2
Spacing: 1.0 in Number of Channels: 3
| DEPTH HDTH TDEP;3

Frame Summary | File: arc_and_sonic_DLIS_Run1__16Sep09_200537__16Sep09_201655 | Sequence: 1 |
Origin: 76
| Index Type | Start | Stop | Spacing | Channels | Index Channel | Frame Name
| BOREHOLE-DEPTH | 150.11 | 816.56 m | 60.0 (0.1 in) down | 71 | TDEP | 60B
|  | 492.50 | 2679.00 ft |  |  |  |
| BOREHOLE-DEPTH | 150.02 | 816.59 m | 12.0 (0.1 in) down | 2 | TDEP;1 | 12B
|  | 492.20 | 2679.10 ft |  |  |  |
| BOREHOLE-DEPTH | 150.01 | 816.61 m | 20.0 (0.1 in) down | 5 | TDEP;2 | 20B
|  | 492.17 | 2679.17 ft |  |  |  |
| BOREHOLE-DEPTH | 150.01 | 816.61 m | 10.0 (0.1 in) down | 3 | TDEP;3 | 10B
|  | 492.17 | 2679.17 ft |  |  |  |

Error Summary | File: arc_and_sonic_DLIS_Run1__16Sep09_200537__16Sep09_201655 | Sequence: 1 |
No errors detected in file.

Schlumberger Verification Listing | Listing Completed: 17-SEP-2009 10:48:00