Schlumberger Verification Listing | Listing Created: 17-SEP-2009 10:48:15 Version: 11C0-208

Input Source: SpikeyBeach1_LWD_RM_RUN2.dlis Format: DLIS Storage Set ID: Default Storage Set | Max Record Length: 8192 Storage Unit Sequence: 1

File Header | File: Quad_Combo_Run2__16Sep09_201326 | Sequence: 1 |
Defining Origin: 121

| File ID: Quad_Combo_Run2__16Sep09_201326 | File Type: CUSTOMER |  |

| Producer Name: Schlumberger | Product/Version: HZ-OP:DnM 1.2.8706.0 | File Set: 1056964608 | File Number: 1 | 16-SEP-2009 20:13:31

Company Name: | Beach Petroleum Ltd
Well Name: | Spikey Beach-1
Field Name: | Exploration

Origin: 122

| File ID: Quad_Combo_Run2__16Sep09_201326 | File Type: CUSTOMER |  |

| Producer Name: Schlumberger | Product/Version: HZ-OP:DnM 1.2.8706.0 | File Set: 1056964608 | File Number: 1 | 16-SEP-2009 20:13:31

Tool String: | DRILLING_SURFACE, ARC8A-AA, MWD_10, SWD8-DA, SADN8-AA
Computations: | ARC8PRESSURECOMPUTATION, ARC8GAMMARAYCOMPUTATION, DENSITY_PROC, NEUTRON_PROC, ULTRASON_PROC

Origin: 123

| File ID: Quad_Combo_Run2__16Sep09_201326 | File Type: CUSTOMER |  |

| Producer Name: Schlumberger | Product/Version: HZ-OP:DnM 1.2.8706.0 | File Set: 1056964608 | File Number: 1 | 16-SEP-2009 20:13:31

Origin: 124

| File ID: Quad_Combo_Run2__16Sep09_201326 | File Type: CUSTOMER |  |

| Producer Name: Schlumberger | Product/Version: HZ-OP:DnM 1.2.8706.0 | File Set: 1056964608 | File Number: 1 | 16-SEP-2009 20:13:31

Tool String: | DRILLING_SURFACE2, ARC9A-AA, SWD9-BA
Computations: | SURVEY, ARC9PRESSURECOMPUTATION, ARC9GAMMARAYCOMPUTATION, ARCRESISTIVITY, WAVEFORMVIEWERENSEMBLE_DNM

Well Site Data | File: Quad_Combo_Run2__16Sep09_201326 | Sequence: 1 |
Origin: 121 Well Data
| Company Name | Beach Petroleum Ltd |  | CN
| Well Name | Spikey Beach-1 |  | WN
| Field Name | Exploration |  | FN
| County: | Australia |  | CLAB, COUN
| State: | Tasmania |  | SLAB, STAT
| Nation | Australia |  | NATI
| Continent | Australasia |  | CONT
| Field Location | Exploration |  | FL
| Service Order Number | 09ASQ0029 |  | SON
| Longitude | 145° 52' 24.71" E |  | LONG
| Latitude | 40° 28' 53.9" S |  | LATI
| Elevation of Ground Level Above Permanent Datum | -74.0 (m) |  | EGL
| Elevation of Derrick Floor Above Permanent Datum | 21.5 (m) |  | EDF
| Permanent Datum | MSL | Elevation of Permanent Datum (PDAT) above Mean Sea Level 0.0 (m) | PDAT, EPD
| Logging Measured From (Name of Logging Elevation Reference) | DF | Elevation of Depth Reference (LMF) Above Permanent Datum 21.5 (m) | LMF, APD
| Drilling Measured From (Name of Drilling Elevation Reference) | DF |  | DMF
Absent Valued Parameters: CN1, FL1, FL2, SECT, TOWN, RANG, APIN, EKB Job Data
| Service Order Number | 09ASQ0029 |  | SON
Absent Valued Parameters: LUN, LUL Origin: 122 (Data differences compared to Origin 121) Well Data
| Maximum Hole Deviation | 0.730 (deg) |  | MHD
Job Data
| Date of Operation | 10-Sep-2009 |  | DATE
| Bottom Log Interval | -999.3 (m) |  | BLI
| Top Log Interval | -999.3 (m) |  | TLI
| Engineer s Name | Marganda Sihite |  | ENGI
| Witness s Name | Fred/Peter |  | WITN
Absent Valued Parameters: RUN Origin: 124 (Data differences compared to Origin 121) Mud Data
| Drilling Fluid Density | 8.80 (lbm/gal) | Drilling Fluid Viscosity 100.0 (s) | DFD, DFV
| Drilling Fluid pH | 9.00 |  | DFPH
| Fluid Interval Transit Time | 206.0 (us/ft) |  | FVEL
| Borehole Salinity | 39794.5 (ppm) |  | BSAL
| Mud Sample Source | Active Tank |  | MSS
| Resistivity of Mud Sample | 0.200 (ohm.m) | Mud Sample Temperature 15.0 (degC) | RMS, MST
| Resistivity of Mud Filtrate Sample | 0.150 (ohm.m) | Mud Filtrate Sample Temperature 20.0 (degC) | RMFS, MFST
| Mudcake Sample Temperature | 20.0 (degC) |  | MCST
| Resistivity of Mud at Bottom Hole Temperature | 0.160 (ohm.m) |  | RMB
| Resistivity of Mud Filtrate At Bottom Hole Temperature | 0.137 (ohm.m) |  | RMFB
Absent Valued Parameters: DFL, RMCS, MRT PVT Data
| Borehole Salinity | 39794.5 (ppm) |  | BSAL
Absent Valued Parameters: ODEN, BO, BW, IBG, BPP, BPT, SGOR

Channels | File: Quad_Combo_Run2__16Sep09_201326 | Sequence: 1 |
Origin: 121 System and Miscellaneous Spacing: 6.0 in Number of Channels: 358
| A112 A114 A122 A124 A132 A134 A142 A144 A152 A154 A16B A16B_COND A16B_COND_UNC A16B_UNC A16H A16H_COND A16H_UNC A16L A16L_COND A16L_UNC A212 A214 A222 A224 A22B A22B_COND A22B_COND_UNC A22B_UNC A22H A22H_COND A22H_UNC A22L A22L_COND A22L_UNC A232 A234 A242 A244 A252 A254 A28B A28B_COND A28B_COND_UNC A28B_UNC A28H A28H_COND A28H_UNC A28L A28L_COND A28L_UNC A34B A34B_COND A34B_COND_UNC A34B_UNC A34H A34H_COND A34H_UNC A34L A34L_COND A34L_UNC A40B A40B_COND A40B_COND_UNC A40B_UNC A40H A40H_COND A40H_UNC A40L A40L_COND A40L_UNC ADIA AMPO AMPR1 AMPR2 AMPR3 AMPR4 ANR1 ANR2 ANR3 ANR4 ANT1 ANT2 ANT3 ANT4 APRS_ARC ATMP BHCX BHCY C1RA C1TA CC15 CC26 CC37 CC48 CDF1 CDF2 CDF3 CDF4 CDF5 CDF6 CDF7 CDF8 CHPO CHRA CHRS CHTA CHTS CL15 CL26 CL37 CL48 CLL2 CLL3 CSL2 CSL3 DCAV DCHO DCRA DCVE DM15 DM26 DM37 DM48 DMXM DPHB DPHI DPHL DPHR DPHU DRHB DRHL DRHO DRHR DRHU DRMS DRSC DSOB DSOL DSOR DSOU DTBC DTPO DTRA DTRS DTSH DTTA DTTS ECD_ARC EFR1 EFR2 FAR1 FAR2 FAR3 FAZ1 FAZ1_R FAZ2 FAZ2_R FAZ3 FAZ3_R GR_ARC GR_ARC_FILT HORD IBT1_ADN IBT2_ADN IDDP IDDQ IDDR IDPE IDQR IDR1 IDR2 IDRO IDU ITTI LSAZ LSHV LSW1 LSW2 LSW3 LSW4 LSW5 LTAZ1 MNS3 MNS4 MNSH MNSL MXS3 MXS4 MXSH MXSL N10V NAZ1 NAZ1_R NAZ2 NAZ2_R NAZ3 NAZ3_R NER1 NER2 NER3 NLTV NPRA NPTA NWRA NWTA P112 P114 P122 P124 P132 P134 P142 P144 P152 P154 P16B P16B_COND P16B_COND_UNC P16B_UNC P16H P16H_COND P16H_UNC P16L P16L_COND P16L_UNC P212 P214 P222 P224 P22B P22B_COND P22B_COND_UNC P22B_UNC P22H P22H_COND P22H_UNC P22L P22L_COND P22L_UNC P232 P234 P242 P244 P252 P254 P28B P28B_COND P28B_COND_UNC P28B_UNC P28H P28H_COND P28H_UNC P28L P28L_COND P28L_UNC P34B P34B_COND P34B_COND_UNC P34B_UNC P34H P34H_COND P34H_UNC P34L P34L_COND P34L_UNC P40B P40B_COND P40B_COND_UNC P40B_UNC P40H P40H_COND P40H_UNC P40L P40L_COND P40L_UNC PEB PEF PEL PER PESC PEU QCDF QIDD QRBB RHOB RHOL RHOS RLSC ROBB ROBL ROBR ROBU ROLB ROLL ROLR ROLU ROP5 ROSB ROSC ROSL ROSR ROSU RPM_ADN RSSC S1RA S1TA SAZ1 SAZ2 SHK1_ADN SHK2_ADN SHKL_FLOAT SOA1 SOA2 SOA3 SOA4 SOA5 SOA6 SOA7 SOA8 SPOR SSHV SSW1 SSW2 SSW3 SSW4 SSW5 STAT_ARC STAZ1 STRA STTA T1RA T1TA TDEP TNPH TNPH_UNC TNRA TNRA_UNC TTPO TTRA TTRS TTTA TTTS U UB UL UOIM UR USC UU VERD WF1G WF1I WF2G WF2I WF3G WF3I WF4G WF4I
Spacing: 1.2 in Number of Channels: 20
| DRSI DSAM LSAZ_P1F NSAM PESI RLSI ROSI ROSI_DYN RSSI SAZ1_P1F SAZ2_P1F TDEP;1 TICKS_CAL TICKS_DEN TICKS_GR TICKS_NEU TICKS_PRES TICKS_RES TICKS_SON USI
Spacing: 2.0 in Number of Channels: 5
| TDEP;2 WF1T WF2T WF3T WF4T
Spacing: 1.0 in Number of Channels: 3
| DEPTH HDTH TDEP;3

Frame Summary | File: Quad_Combo_Run2__16Sep09_201326 | Sequence: 1 |
Origin: 121
| Index Type | Start | Stop | Spacing | Channels | Index Channel | Frame Name
| BOREHOLE-DEPTH | 803.15 | 2100.38 m | 60.0 (0.1 in) down | 358 | TDEP | 60B
|  | 2635.00 | 6891.00 ft |  |  |  |
| BOREHOLE-DEPTH | 803.03 | 2100.38 m | 12.0 (0.1 in) down | 20 | TDEP;1 | 12B
|  | 2634.60 | 6891.00 ft |  |  |  |
| BOREHOLE-DEPTH | 803.05 | 2100.38 m | 20.0 (0.1 in) down | 5 | TDEP;2 | 20B
|  | 2634.67 | 6891.00 ft |  |  |  |
| BOREHOLE-DEPTH | 803.02 | 2100.38 m | 10.0 (0.1 in) down | 3 | TDEP;3 | 10B
|  | 2634.58 | 6891.00 ft |  |  |  |

Error Summary | File: Quad_Combo_Run2__16Sep09_201326 | Sequence: 1 |
No errors detected in file.

Schlumberger Verification Listing | Listing Completed: 17-SEP-2009 10:48:18