area  name::  HOWARDS
who  survey  for::  C.R.A.  EXPLORATION
who  performed  by::  BM  TC  PMM
job  number::  8603
  4  digit  loop  number::  0002
  +x  symbol::  E
 +y  symbol::  N
  +z  symbol::  U
M+1::  46
N+1024::  1036
  freq::    2.622964E1
E dipole  length::    1.000000
  name  of  file  of  calibration  data::  NOMCAL2
distance  unit  per  metre::    1.000000
#  of  corners  of  loop::  4
  cor  #    x        y          z
1  1.000010E3  2.500100E2  1.000000E-2
2  1.600010E3  1.000100E2  1.000000E-2
3  1.600010E3  1.500010E3  1.000000E-2
4  1.000010E3  1.650010E3  1.000000E-2
smallest  line  #::  18
corresponding  nominal  y  value::    1.000000E2
largest  line  #::  23
corresponding  nominal  y  value::    1.250000E3
#  of  lines::  6
smallest  label::  1625
corresponding  nominal  x  value::    1.625000E3
largest  label::  2700
corresponding  nominal  x  value::    2.700000E3
#  of  stations  per  line::  44
**  plot  options  **
max  chan  to  plot::  10
chan  to  repeat  if  multi  axis  plot::  5
number  of  separate  axes::  3  
  top  of  top  axis::    9.468501E1
  zero  top  axis::    7.500000E1
  bot  of  top  axis::    5.531500E1
  scale  of  top  axis::    5.080000
  number  of  ticks  top  axis::  11
  top  of  centre  axis::    4.984250E1
  zero  centre  axis::    4.000000E1
  bot  of  centre  axis::    3.015750E1
  scale  of  centre  axis::    1.016000
  number  of  ticks  centre  axis::  11
  top  of  bottom  axis::    2.484250E1
  zero  bottom  axis::    1.500000E1
  bot  of  bottom  axis::    5.157500
  scale  bottom  axis::    2.540000
  no.  of  ticks  bottom  axis::  11
  xscale::    1.270000E1
  centre  of  plot  area::    7.000000E1
labelling  unit  for  x  axis::    1.000000E2
number  of  trailing  zeroes  to  delete::  2
station  x  value  at  y  axis::    1.600000E3
station  x  value  of  leftmost  point  on  plot::    1.625000E3
station  x  value  of  rightmost  point  on  plot::    2.600000E3
