area name::  PASMINCO MINE
client name::  PASMINCO EXPLOATION
performed by::  LAMONTAGNE GEOPHYSICS LTD
job number::  9105
4 digit loop number:: SE02
+x symbol::  E
+y symbol::  N
+z symbol::  U
M+1::  45
N+1025::  1059
freq::  2.6230E1
E dipole length::  2.5000E1
calibration file name::  NOMCAL
distance per unit metre::  1.0000
# of corners of loop::       12
 cor #  x    y     z
       1  9.7500000e+3    -8.1500000e+2     0.0000000e+0   
       2  9.7612939e+3    -5.8144379e+2     0.0000000e+0   
       3  9.7330000e+3    -3.0000000e+2     0.0000000e+0   
       4  9.7270000e+3     0.0000000e+0     0.0000000e+0   
       5  9.7180000e+3     3.5000000e+2     0.0000000e+0   
       6  9.7180000e+3     7.0000000e+2     0.0000000e+0   
       7  9.0500000e+3     7.5000000e+2     0.0000000e+0   
       8  8.8500000e+3     3.5000000e+2     0.0000000e+0   
       9  8.8600000e+3     0.0000000e+0     0.0000000e+0   
      10  9.1350000e+3    -5.7000000e+2     0.0000000e+0   
      11  9.3445742e+3    -7.9145789e+2     0.0000000e+0   
      12  9.5074111e+3    -8.6427692e+2     0.0000000e+0   
smallest line label #::  1
corresponding nominal y value:: -3.700e+2   
largest line label::  4
corresponding nominal y value::  462   
the number of lines::  4
smallest station label::  3800
corresponding x value::  8.800e+3   
largest station label::  6300
corresponding x value::  1.130e+4   
the number of stations::  51
** plot options **
max chan to plot::  10
chan to repeat if multi axis plot::  5
number of separate axes::  3
top of top axis::  94.68501
zero of top axis::  75.0
bottom of top axis::  55.315
scale of top axis::  5.08
number of tics on top axis::  11
top of centre axis::  49.8425
zero of centre axis::  40.0
bottom of centre axis::  30.1575
scale of centre axis::  2.54
number of tics on centre axis::  11
top of bottom axis:: 24.8425
zero of bottom axis::  15
bottom of bottom axis::  5.1575
scale of bottom axis::  2.54
number of tics on bottom axis::  11
x-scale::  1.27
centre of plot area::  70
labelling interval for x-axis::  200
number of trailing zeros to delete::  0
x-value at the y-axis::  8.8000E3
x-value at leftmost point on plot::  8.8000E3

