area name::  MACKINTOSH
client name::  ABERFOYLE RESOURCES
performed by::  LAMONTAGNE GEOPHYSICS LTD
job number::  9309
4 digit loop number:: 2
+x symbol::  E
+y symbol::  N
+z symbol::  U
M+1::  27
N+1025::  1059
freq::  4.372E1
E dipole length::  2.5000E1
calibration file name::  cal10
distance per unit metre::  1.0000
how many vertices::  4
cor #       x       y         z
	1	4900 5800 0
	2	4900 6200	0
	3	4500 6200	0
	4	4500 5800	0
smallest line label #::  28
corresponding nominal y value::  28  
largest line label::  28
corresponding nominal y value::  28  
the number of lines::  0
smallest station label::  0
corresponding x value::  0   
largest station label::  0
corresponding x value::  0   
the number of stations::  0
** plot options **
max chan to plot::  10
chan to repeat if multi axis plot::  5
number of separate axes::  3
top of top axis::  94.68501
zero of top axis::  75.0
bottom of top axis::  55.315
scale of top axis::  5.08
number of tics on top axis::  11
top of centre axis::  49.8425
zero of centre axis::  40.0
bottom of centre axis::  30.1575
scale of centre axis::  2.54
number of tics on centre axis::  11
top of bottom axis:: 24.8425
zero of bottom axis::  15
bottom of bottom axis::  5.1575
scale of bottom axis::  2.54
number of tics on bottom axis::  11
x-scale::  1.27
centre of plot area::  70
labelling interval for x-axis::  200
number of trailing zeros to delete::  0
x-value at the y-axis::  1.8000E2
x-value at leftmost point on plot::  1.8000E2
x-value at the rightmost point on plot::  5.2000E2
