DataSet	Hole_ID	Hole_Type	Extension_Type	Wedge_Depth	Parent_Hole_ID	Year	EOH	Ref_System	Ref_Method	Ref_Accuracy	UTM_East	UTM_North	UTM_RL	UTM_Grid	Lat	Long	LL_Datum	Local_East	Local_North	Local_RL	Local_Grid_Name	Project	Prospect	Tenement_No	Date_Commenced	Date_Completed	Casing_Type	Casing_Depth_From	Casing_Depth_To	Casing_Diameter	Watertable_Depth_m	Groundwater_Quality	Company	Drilling_Company	Drill_Rig	Logged_By	Sampled_By	Purpose	Termination_Reason	Mineralisation	Best_Intersections	Data_Source	Rehab	Comments
DUNDAS	CP353	DD				2004	905.5	UTM	DGPS	5	377163.2	537133.2	249.4	AMG66_55								DUNDAS	Chamberlain	EL 11/2002	17/03/2004	29/04/2004	PVC	0	905.5	40mm			Zinifex	Boart Longyear	UDR650	AMcN	CA/RA	Test Chamberlain deep EM anomaly	Reached rig capacity - no obvious source for EM anomaly.				site yet to be rehabilitated.	
