Two copies of DVD’s were prepared.

There are two (2) main directories,

	Data		contains a database, grids and maps, as described below. 
			 
	Report	            contains a copy of the report and appendices in Microsoft Word      format.

•	Database for each area are in Geosoft GDB format, and contain the following channels:

X:		X positional data (metres – GDA94, AMG Zone 55 South)
Y:		Y positional data (metres – GDA94, AMG Zone 55 South)
Lon:		Longitude data (degree – GDA94)
Lat:		Latitude data (degree – GDA94)
Z:		GPS antenna elevation (metres - ASL)
Gtime:		UTC time (seconds of the day)
Basemag:	Base magnetic diurnal variations (nT)
Radarb:         EM Transmitter and Receiver terrain clearance (metres - AGL)
DEM:		Digital elevation model (metres)
Mag1:		Raw Total Magnetic field data (nT)
Mag2:		Total Magnetic field diurnal variation corrected data (nT)
Mag3:		Levelled Total Magnetic field data (nT)
SF:		dB/dt array channel

SF[8]:	dB/dt 83 microsecond time channel (pV/A/m4)
SF[9]:	dB/dt 99 microsecond time channel (pV/A/m4)
SF[10]:	dB/dt 120 microsecond time channel (pV/A/m4)
SF[11]:	dB/dt 141 microsecond time channel (pV/A/m4)
SF[12]:	dB/dt 167 microsecond time channel (pV/A/m4)
SF[13]:	dB/dt 198 microsecond time channel (pV/A/m4)
SF[14]:	dB/dt 234 microsecond time channel (pV/A/m4)
SF[15]:	dB/dt 281 microsecond time channel (pV/A/m4)
SF[16]:	dB/dt 339 microsecond time channel (pV/A/m4)
SF[17]:	dB/dt 406 microsecond time channel (pV/A/m4)
SF[18]:	dB/dt 484 microsecond time channel (pV/A/m4)
SF[19]:	dB/dt 573 microsecond time channel (pV/A/m4)
SF[20]:	dB/dt 682 microsecond time channel (pV/A/m4)
SF[21]:	dB/dt 818 microsecond time channel (pV/A/m4)
SF[22]:	dB/dt 974 microsecond time channel (pV/A/m4)
SF[23]:	dB/dt 1151 microsecond time channel (pV/A/m4)
SF[24]:	dB/dt 1370 microsecond time channel (pV/A/m4)
SF[25]:	dB/dt 1641 microsecond time channel (pV/A/m4)
SF[26]:	dB/dt 1953 microsecond time channel (pV/A/m4)
SF[27]:	dB/dt 2307 microsecond time channel (pV/A/m4)
SF[28]:	dB/dt 2745 microsecond time channel (pV/A/m4)
SF[29]:	dB/dt 3286 microsecond time channel (pV/A/m4)
SF[30]:	dB/dt 3911 microsecond time channel (pV/A/m4)
SF[31]:	dB/dt 4620 microsecond time channel (pV/A/m4)
SF[32]:	dB/dt 5495 microsecond time channel (pV/A/m4)
SF[33]:	dB/dt 6578 microsecond time channel (pV/A/m4)
SF[34]:	dB/dt 7828 microsecond time channel (pV/A/m4)
PLM:		Power line monitor
  
 
•	Database A353_Waveform.gdb in Geosoft GDB format, containing the following channels:

Time:		Sampling rate interval, 10.416 microseconds
Volt:		Output voltage of the receiver coil (volt)

•	Maps for each area at 1:10,000 scale in Geosoft MAP & MapInfo TAB formats, are as follows:
 
A353_1_EMLog_SF_Survey:	dB/dt profiles at a logarithmic scale for all survey lines E-W, time channels 0.1– 9.24 ms

A353_1_EMLog_SF_Survey_Infills:	dB/dt profiles at a logarithmic scale 
for all infill lines E-W, time channels 
0.1 – 9.24 ms

A353_1_Mag3:		Total magnetic intensity contours and 
colour image

A353_1_DEM:		Digital elevation model contours and 
colour image

A353_1_FP:		Flight path

A353_2_EMLog_SF_Survey:	dB/dt profiles at a logarithmic scale for all survey lines NE-SW, time channels 0.1– 9.24 ms

A353_2_Mag3:		Total magnetic intensity contours and 
colour image

A353_2_DEM:		Digital elevation model contours and 
colour image

A353_2_FP:		Flight path


•	Google Earth file A353_1_ Heazle _Flightplan_Google.kml and A353_2_RHILL_Flightplan_Google.kml show the flight path of the blocks 1 and 2

Free version of Google Earth software can be downloaded from

http://earth.google.com/download-earth.html
