SCINTREX VLF-4 data

Acquired by RGC Exploration staff in 1996

Transmitter: NW Cape 22.3kHz

All field dump files have extension .RAW

EXCEL spreadsheet file vlf_data.xls contains simple processing algorithms (such as FRAZER filtering)

Columns in VLF_DATA.LIN are as follows:

Line     East     North    Vertical In-Phase     Vertical Out-of-Phase     Horizontal Field Component