MetaData Begin
	Name	= AA926_Frontier_Daguilar_Final_BFz_Band30.ers
	Version	= 396
	AA926_Frontier_Daguilar_Final_BFz_Band30 Begin
		GroupBy	= no
		DataType	= IEEE4ByteReal
		ByteOrder	= LSBFirst
		Bands	= 1
		Minimum	= -0.0197220761329
		Maximum	=  0.078150652349
		Mean	= 0.00211994467778
		Variance	= 2.72935301651e-005
		Samples	= 43519
		Nulls	= 18837
		Projection	= "MGA55"
		Datum	= "WGS84"
		BandId	= "0.880ms"
	AA926_Frontier_Daguilar_Final_BFz_Band30 End
	Creation_History Begin
		Process Begin
			Name	= GriddingPro
			Parameters Begin
				Input_Datasets Begin
					Input_Dataset_1 Begin
						Input_Dataset	= X:\00TCR\12_6461working\Daguilar\OriginalData\AA926_Frontier_Daguilar_Final.gdb
						Input_X	= x_MGA
						Input_Y	= y_MGA
						Data	= BFz
						Band	= 30
						Survey_Lines Begin
							LineType	= GS_LType
						Survey_Lines End
					Input_Dataset_1 End
				Input_Datasets End
				Grid_Refinement Begin
					Fill_Holes	= no
					Edge_Clipping	= Extrapolation_limits
					Laplace_Iterations	= 2
				Grid_Refinement End
				Output_Grid Begin
					Output_Grid	= X:\00TCR\12_6461working\Daguilar\OriginalData\AA926_Frontier_Daguilar_Final_BFz_Band30.ers
					Datum	= WGS84
					Projection	= MGA55
					Cell_Size_X	= 37.500000
					Cell_Size_Y	= 37.500000
					Band	= 1
					Band_Name	= 0.880ms
					Bands	= 1
					DataType	= IEEE4ByteReal
					Rotation	= 0.0
					Null_Value	= -99999.0
					Origin_X	= 383960.000000
					Origin_Y	= 5285120.000000
					Columns	= 131
					Rows	= 476
				Output_Grid End
				Gridding_Method Begin
					Extrapolation_Limit	= 5
					Cell_Assignment	= Closest
					Name	= BiCubic_Spline
					Min_Scan_Distance	= 0.0
					Max_Scan_Distance	= 2000.0
					Spline_Type	= Akima
					Spline_Gradient_Signal-Noise_Blending	= no
					Spline_Gradient_Noise_Level	= 0.01
				Gridding_Method End
			Parameters End
			Comments	= "Intrepid Audit Stamp v4.2.3 Release for Windows (x86) by SUNFIRE Build 396 - 3/ 7/2012"
		Process End
	Creation_History End
MetaData End
