                                                    

                                                                           

    MINERAL CHEMISTRY     Amdel Laboratories Ltd      Telephone (08) 8416 5300

                                PO Box 338            Facsimile (08) 8234 0321

                         Torrensville Plaza SA 5031

                             ACN 009 076 555







    Mr Anthony Jannink                      

    Jervois Mining NL                       

    4th Floor, 114 William Street           

    MELBOURNE   VIC   3000                  

                                            







                          FINAL ANALYSIS REPORT





    Your Order No: G50834                     Our Job Number :  1AD0217        





    Sample rec'd :     31/01/01             Results reported :  14/02/01



    No. of samples      :     3      



    Results apply to sample(s) as submitted by client.



    Report comprises a cover sheet and pages:  1 to 2                                  







    Approved:



    

    Alan Ciplys

    Manager, Geoanalytical, Eastern Australia





                                                      

                                                      





    Report  Codes:                                  Distribution Codes:

    N.A.   - Not Available.                         CC    -  Carbon Copy

    L.N.R. - Listed But Not Received.               EM    -  Electronic Media

    I.S.   - Insufficient Sample.                   MM    -  Magnetic Media



  

                          ***   Please Note   ***



1) The results for elements 'Al, Ba, Cr, Ti, W, Zr, Sn' by code IC3E digest

      are acid soluble only, and results may be semi-quantative.

   'K' values >1% by code IC3E may bias low due to the insolubility

      of potassium perchlorate.



2) Total 'Fe' is analysed but is calculated and reported as 'Fe2O3'



3) The Scheme WAMBM involves the analysis of `mobile metals ions' by the

      `WAMTECH' partial digest technique using leach solution `B'.

   The Scheme WAMAM involves the analysis of `mobile metals ions' by the 

      `WAMTECH' partial digest technique using leach solution `A'.



                                                    Job: 1AD0217

                                                    O/N: G50834

Final                          ANALYTICAL REPORT



              SAMPLE        Co     Ni     Sc     Al     Cr     Fe     Mg



                  B1     0.025  0.090     35   10.6   1.28   29.4   0.20

                  B2     0.100  0.100     35   14.5   0.69   17.3   0.29

                  K1        --     --     --     --     --     --     --

































































































               UNITS         %      %    ppm      %      %      %      %

             DET.LIM     0.005  0.005      5   0.01   0.01    0.1   0.01

              SCHEME      IC3B   IC3B   IC3B   IC3B   IC3B   IC3B   IC3B



                                                           Page   1 of   2



                                                    Job: 1AD0217

                                                    O/N: G50834

Final                          ANALYTICAL REPORT



              SAMPLE        Au Au Rpt     Mn     Ca     Cu     Pb     Zn



                  B1        --     --   0.15    750     <5    <10    135

                  B2        --     --   0.41   1450      5    <10     90

                  K1     <0.01  <0.01     --     --     --     --     --

































































































               UNITS       ppm    ppm      %    ppm    ppm    ppm    ppm

             DET.LIM      0.01   0.01   0.01     20      5     10      5

              SCHEME       FA1    FA1   IC3B   IC3B   IC3B   IC3B   IC3B



                                                           Page   2 of   2

