                                                    
                                                                           
    MINERAL CHEMISTRY     Amdel Laboratories Ltd      Telephone (08) 8416 5300
                                PO Box 338            Facsimile (08) 8234 0321
                         Torrensville Plaza SA 5031
                             ACN 009 076 555



    Mr Anthony Jannink                      
    Jervois Mining NL                       
    4th Floor, 114 William Street           
    MELBOURNE   VIC   3000                  
                                            



                          FINAL ANALYSIS REPORT


    Your Order No: G50834                     Our Job Number :  1AD0217        


    Sample rec'd :     31/01/01             Results reported :  14/02/01

    No. of samples      :     3      

    Results apply to sample(s) as submitted by client.

    Report comprises a cover sheet and pages:  1 to 2                                  



    Approved:

    
    Alan Ciplys
    Manager, Geoanalytical, Eastern Australia


                                                      
                                                      


    Report  Codes:                                  Distribution Codes:
    N.A.   - Not Available.                         CC    -  Carbon Copy
    L.N.R. - Listed But Not Received.               EM    -  Electronic Media
    I.S.   - Insufficient Sample.                   MM    -  Magnetic Media

  
                          ***   Please Note   ***

1) The results for elements 'Al, Ba, Cr, Ti, W, Zr, Sn' by code IC3E digest
      are acid soluble only, and results may be semi-quantative.
   'K' values >1% by code IC3E may bias low due to the insolubility
      of potassium perchlorate.

2) Total 'Fe' is analysed but is calculated and reported as 'Fe2O3'

3) The Scheme WAMBM involves the analysis of `mobile metals ions' by the
      `WAMTECH' partial digest technique using leach solution `B'.
   The Scheme WAMAM involves the analysis of `mobile metals ions' by the 
      `WAMTECH' partial digest technique using leach solution `A'.

                                                    Job: 1AD0217
                                                    O/N: G50834
Final                          ANALYTICAL REPORT

              SAMPLE        Co     Ni     Sc     Al     Cr     Fe     Mg

                  B1     0.025  0.090     35   10.6   1.28   29.4   0.20
                  B2     0.100  0.100     35   14.5   0.69   17.3   0.29
                  K1        --     --     --     --     --     --     --
















































               UNITS         %      %    ppm      %      %      %      %
             DET.LIM     0.005  0.005      5   0.01   0.01    0.1   0.01
              SCHEME      IC3B   IC3B   IC3B   IC3B   IC3B   IC3B   IC3B

                                                           Page   1 of   2

                                                    Job: 1AD0217
                                                    O/N: G50834
Final                          ANALYTICAL REPORT

              SAMPLE        Au Au Rpt     Mn     Ca     Cu     Pb     Zn

                  B1        --     --   0.15    750     <5    <10    135
                  B2        --     --   0.41   1450      5    <10     90
                  K1     <0.01  <0.01     --     --     --     --     --
















































               UNITS       ppm    ppm      %    ppm    ppm    ppm    ppm
             DET.LIM      0.01   0.01   0.01     20      5     10      5
              SCHEME       FA1    FA1   IC3B   IC3B   IC3B   IC3B   IC3B

                                                           Page   2 of   2
