HOLE ID	mFROM	mTO	INTERVAL	COMMENTS	MINERALISATION	ALTERATION
MODD01	0.00	1.00	1.00	"SURFICIAL ZONE, BASALTIC SOIL AND RUBBLE."		
MODD01	1.00	5.40	4.40	"BASALT. STRONGLY WEATHERED ZONE IN AUTOBRECCIATED BASALT FLOW. SUB-ANGULAR
TO SUB-ROUNDED BASALTIC CLASTS AND GLASS IN ORANGE PIEZOLITIC-LOOKING 
MATRIX. CLASTS  <10CM."		BLUE-GREEN OXIDE COATING ON SOME JOINT/FRACTURE SURFACES-PROBABLY IRON OXIDES.
MODD01	5.40	14.90	9.50	"AUTOBRECCIATED BASALTIC FLOW. MODERATE TO WEAKLY WEATHERED. ANGULAR
 TO SUB-ROUNDED CLASTS UP TO 20CM. SUPPORTED IN A CHLORITISED GLASS-RICH
MATRIX. CLASTS OLIVINE-RICH."		
MODD01	14.90	17.40	2.50	"DEEP LEAD MATERIAL. 
STRONGLY CLAY WEATHERED ROCK ?AFTER WRIGGLITE. GENERALLY NON-MAGNETIC
GREY-WHITE TO YELLOW-BROWN CONTACT METAMORPHOSED CLAYS."	? MAY CONTAIN TIN AND TUNGSTEN.	
MODD01	17.40	24.10	6.70	"WEATHERED WRIGGLITE.
ZONE OF KAOLINITIC AND FE OXIDE WEATHERING. KAOLINITE IN FRACTURES AND
ALTERATION AT VEINS. WRIGGLITE TEXTURES EASILY VISIBLE. PROBABLE FAULT AT
23.4M OVER 30CM, VERY BROKEN."		
MODD01	24.10	38.60	14.50	"FRESH WRIGGLITE.
90-95% MAGNETITE-FLOURITE WRIGGLITE WITH ~5% DISJOINTED LENSES/PATCHES OF
CALC-SILICATE.
VEINING WEAK, INCREASING TO MODERATE DOWNHOLE THREAD-LIKE TO CM SCALE
STOCKWORK OF PINK-WHITE QUARTZITE. SOME VEINS HAVE MAGNETITE-RICH
SELVEDGES."	TRACE PYTITE/PYRRHOTITE COATINGS ON SOME FRACTURE SURFACES.	"MODERATE CHLORITE FROM 29.4 M=PATCHY ALTERATION OF CALC-SILICATE, WEAK EPIDOTE THROUGHOUT."
MODD01	38.60	45.40	6.80	"MIXED WRIGGLITE/CALC SILICATE.
~30% PATCHY MAGNETITE-RICH WRIGGLITE WITH CREAM TO GREEN-WHITE
CALC-SILICATE. MODERATE CM SCALE VEINING WITH REDDISH PINK TO WHITE
QUARTZITE. SEVERAL CROSS-CUTTING VEIN SETS, SOME WITH MAGNETITE-RICH
SELVEDGES PLUS FINE DARK MINERAL IN VEIN CORES. ?VEINS MAY BE TOPAZ OR
RHODONITE-RICH , VERY HARD."		"WEAK CHLORITE-EPIDOTE, PERVASIVE."
MODD01	45.40	50.40	5.00	"WRIGGLITE.  80% WRIGGLITE, VERY MAGNETITE-RICH WITH LESS DISTINCT FLOURITE
LAMINATIONS THAN ABOVE.
SHEARED CONTACTS EVIDENT ON EITHER SIDE OF THIS ZONE.
MODERATE VEINING AS ABOVE."	"43.3-45.3M RUBBLE, FAULT ZONE SHEARED, CHLORITISED.
48.9-51.4M RUBBLE, FAULT ZONE SHEARED, CHLORITISED."	VERY MAGNETITE-RICH.
MODD01	50.40	62.00	11.60	"CALC-SILICATE SKARN-MAGNETITE POOR. CREAM-GREEN, FINE-GRAINED REDDISH
GARNET-RICH, VERY HARD.
MODERATE CM SCALE QTZ-FLUORITE ?VEINING WITH DISTINCT MM SCALE MAGNETITE-RICH SELVEDGES. GRADATIONAL CONTACTS OVER 1M."		"PATCHY CLOTS OF CHLORITE, INTENSE GARNET."
MODD01	62.00	71.00	9.00	"PATCHY WRIGGLITE/CALC-SILICATE SKARN.  50% WRIGGLITE VERY HARD, GARNET-RICH
30CM VEIN/PATCH OF CRYSTALLINE  <MM  SCALE MAGNETITE-GARNET-EPIDOTE -
CHLORITE WITH TRACE MOLYBDENITE AT 64.3M.
MODERATE CM SCALE RED-PINK AND WHITE FINE GRAINED SILICATE VEINS.
VERY HARD, NO SELVEDGES.
"	"TRACE MOLYBDENITE, POSSIBLE TRACE WOLFRAMITE AT 64.3M."	
MODD01	71.00	83.40	12.40	"GARNET-RICH CALC-SILICATE SKARN, AS AT 50.4M."		
MODD02	0.00	2.00	1.00	"PROBABLE BASALT, RED GARNET IMPREGNATED.  10CM PALAEOSOIL CLAY AT 1.9M.
FINE-GRAINED REDDISH-BLACK, HARD, NON-MAGNETIC BASALTIC LOOKING ROCK."		
MODD02	2.00	7.40	5.40	"WEATHERED WRIGGLITE SKARN.
ORANGE-BROWN AND WHITE CLAY DEVELOPMENT. STRONGLY WEATHERED TO 5.4M,
MODERATELY WEATHERED TO 7.4M.
"		
MODD02	7.40	11.40	4.00	"WRIGGLITE SKARN-WEAKLY WEATHERED.
CLAY AND OXIDE DEVELOPMENT IN FRACTURES.
STRONGLY MAGNETIC MAGNETITE-FLOURITE SKARN.  MODERATE PINK QUARTZ-?FLUORITE
VEINING TO 1CM "	90%+ WRIGGLITE MATERIAL	
MODD02	11.40	17.40	6.00	"FRESH WRIGGLITE SKARN.
MAGNETITE-FLOURITE WRIGGLITE WITH UP TO 2MM FLUORSPAR LAMINATIONS.
2-3% PYRITE/PYRRHOTITE FROM 15.5-17.4M."	"50% MAGNETITE, 40% FLUORSPAR, 70% QUARTZ VEINING, 1-3% PYRRHOTITE/PYRITE."	
MODD02	17.40	18.00	0.60	"BLACK CLAYS-PROBABLE FAULT. TRANSITION ZONE
CALC-SILICATE DOMINANT ZONE  <10% WRIGGLITE.  NO NOTABLE SULPHIDES. "	~5% WRIGGLITE.	
MODD02	18.00	28.20	10.20	"CALC-SILICATE SKARN. 
REDDISH-CREAM SKARN ROCK WITH PATCHY LENSES OF SILTY MATERIAL.
INCREASING GARNET ALTERATION DOWNHOLE TO GARNET DOMINANT WITH MINOR
TOURMALINE.
VISIBLE RED GARNET CRYSTALS AT 25M."		"INTENSE GARNET, MINOR TOURMALINE-EPIDOTE."
MODD02	28.20	30.70	2.50	"RUBBLE ZONE-PROBABLE FAULT.
QTZ-FLUORSPAR VEINING TO 10CM WITH MAGNETITE SELVEDGES.
"		
MODD02	30.70	45.30	14.60	"GARNET-DOMINANT SKARN.
REDDISH-CREAM FINE GRAINED  (<1MM) RED GARNET DOMINANT ROCK WITH 
OCCASIONAL TOURMALINE CLOTS AND DISSEMINATED MINOR EPIDOTE.
WEAK QUARTZ-FLOURITE-MAGNETITE VEINING TO 10CM WITH UP TO 5%  MOLYBDENITE IN VEINS.
POSSIBLE TRACE BISMUTHENITE AT 39.3M. 10CM QUARTZ-FELDSPAR-FLUORITE VEIN WITH MUSCOVITE AT 41.7M."	TRACE MOLYBDENITE AND POSSIBLE BISMUTHENITE.	
MODD02	45.30	46.00	0.70	"SILICEOUS CHERTY GREY-GREEN SPOTTY CALC-SILICATE ROCK.  MODERATE
THREAD-LIKE DARK GREEN TO BROWN VEINLETS ?PYROXENE AND QUARTZ-FLOURITE 
MM SCALE."	5% WOLFRAMITE IN QUARTZ-FLOURITE-MOLYBDENITE VEIN AT 35.6M.	
MODD02	46.00	53.40	7.40	"GREY SILICEOUS FINE-GRAINED CALC-SILICATE ROCK? ALTERED LIMESTONE.
HIGHLY FRACTURED AND MODERATE ORANGE-BROWN TO GREY CLAY ALTERATION.
LOCALLY 5% MOLYBDENITE IN FRACTURES AT 52.3M."	TRACE MOLYBDENITE OVERALL. TRACE WOLFRAMITE IN SILICATE VEINS.	
MODD02	53.40	65.40	12.00	"SHEAR ZONE.
STRONGLY FRACTURED, RUBBLY, STRONGLY CLAY ALTERED.
GREENISH-GREY, SHEARED CALC-SILICATE ROCK.  
DISTINCTIVE YELLOW SOFT ?ZEOLITE ALTERATION THROUGHOUT. SEVERAL LIKELY FAULT ZONES WITH BRECCIATION AND CLAYS AT 51.4M, 53.5M, 56.0M AND 57.8 M. 10CM QUARTZ-FELDPSAR-FLOURITE VEIN WITH MUSCOVITE AT 41.7M."	MINOR WOLFRAMITE AT 57.7M.	
MODD03	0.00	1.60	1.60	"* DDH COLLORED ON OLD MILL ACCESS TRACK.
SURFICIAL PYRITIC ROAD BASE AND BROWN CLAYS."		
MODD03	1.60	3.10	1.50	"WEATHERED ZONE OF BRECCIATED BASALTIC MATERIAL.
STRONG FE-OXIDE (HEMATITE, LIMONITE, MANGANESE OXIDE) DEVELOPMENT. INCLUDES SLIGHTLY
WEATHERED BASALTIC CLASTS UP TO 10CM."		
MODD03	3.10	5.80	2.70	"BRECCIATED BASALT. LIKELY AUTOBRECCIATED BASALTIC FLOW.  HIGHLY ANGULAR 
BASALTIC CLASTS AND SCATTERED OLIVINE TO 10CM IN CHLORITISED ?ASHY MATRIX.
STRONGLY CHLORITISED AND FINE-GRAINED OVER 30CM AT BASAL CONTACT ?ASH UNIT AT BASE SHARP LOWER CONTACT."	TRACE FINE-GRAINED PYRITE AND BLUE-GREY OXIDE DEVELOPMENT IN VUGS AND ON FRACTURE SURFACES.	STRONG CHLORITE.
MODD03	5.80	6.00	0.20	"DEEP LEAD. TERTIARY PALAEOSURFACE GRAVELS. INDURATED QUARTZ SANDSTONE
QUARTZITE GRAVELS.  QUARTZITE PEBBLES UP TO 4CM DIAMETER."		
MODD03	6.00	7.70	1.70	"DOMINANTLY BLUE-BLACK CLAYS  STRONGLY MAGNETIC?, MAGNETITE 
CONCENTRATED IN PALAEOSURFACE.  WEATHERING PROFILE INCLUDES 10CM OF BLACK AND
CREAM LAMINATED WEATHERED ROCK AT 6.4M (?WRIGGLITE). GRADATION DOWNHOLE TO 
RED-BLACK CLAYS?"	PYRITIC 1CM VUGS IN WEATHERED CLAST AT 6.4M.	
MODD03	7.70	11.00	3.30	"RED TO YELLOW CLAY-DOMINATED WEATHERING ZONE WITH OCCASIONAL
RELICT WRIGGLITE TEXTURES.  MINOR WHITE CLAYS.
PATCHES OF STRONGLY MAGNETIC MATERIAL ASSOCIATED WITH RED FE-OXIDE CLAYS. WEATHERED SKARN."	WEATHERING-FE OXIDES. NO SULPHIDES OBSERVED. 	
MODD03	11.00	21.10	10.10	"WEATHERED SKARN. ZONE OF WHITE KAOLINITIC CLAY ALTERATION IN VARIABLY STRONGLY MAGNETIC WEATHERED SKARN.
BRECCIATED TEXTURE WITH DARK MAGNETIC CLASTS ~2CM WITH KAOLINITIC MATRIX
11.8-12.2M. SOME WRIGGLITE TEXTURES EVIDENT.
RUBBLE ZONE 15.8-18.8M MAY BE A FAULT ZONE. 18.8-21.1M GRADATIONAL CORE COMPLETENCE INCREASE TO MODERATE-STRONG KAOLINITE-CHLORITE ALTERATION OF WRIGGLITE SKARN.  KAOLINITE, DOMINANTLY ALTERS 1MM-1CM VEIN NETWORKS. MAGNETITE-FLUORSPAR BONDING EVIDENT."		STRONG KAOLINITE IN SKARN AND IN VEINS. MODERATE-STRONG CHLORITE±EPIDOTE? OF WRIGGLITE MAGNETITE.
MODD03	21.10	26.30	5.20	"WEAK-MODERATELY WEATHERED, MODERATELY CHLORITE-KAOLINITE ALTERED.
MIXED CALC-SILICATE-WRIGGLITE-SKARN.
APPROX 20% STRONGLY MAGNETIC WRIGGLITE, 80% BLOTCHY TO SPOTTY 
CHLORITE-KAOLINITE ALTERED ROCK WITH THREAD-LIKE TO 1CM KAOLINITE ALTERED?
ADULARIA VEIN STOCKWORK. CROSS-CUTTING VEIN SETS EVIDENT. MOSTLY 60-80 DEGREES/VCA."	1% FINE BRASSY TO COPPER COLOURED SULPHIDE OVER 10CM AT 25.4M (NOT PYRITE OR CHALCOPYRITE).	
MODD03	26.30	27.80	1.50	"STRONGLY CHLORITISED RUBBLE ZONE -PROBABLE FAULT IN MIXED WRIGGLITE/ 
CALC-SILICATE SKARN."		
MODD03	27.80	29.90	2.10	"PALE CREAM-GREEN WEAKLY CHLORITE ALTERED MARBLE/CALC-SILICATE WITH 
THREAD TO 2CM HEALED VEINLET STOCKWORK."	?SCHEELITE IN VEINS?	
MODD03	29.90	34.60	4.70	"DARK PURPLISH-GREEN MOTTLED, MODERATELY CHLORITISED STRONGLY MAGNETIC
WRIGGLITE SKARN.
MODERATE SINUSOIDAL TO STOCKWORK VEINING MOSTLY 0.5CM.
WHITE TO PINKISH PROBABLE CLAY ALTERED FELDSPAR WITH OCCASIONAL MAGNETITE-RICH SELVEDGES AND MINOR CHLORITE/EPIDOTE .
SCHEELITE CONTENT UNKNOWN. VEINING AT LOW ANGLE TO VCA DOMINANTLY, BUT BECOMING STRONG IN FREQUENCY AT 60-70 DEGREES TO VCA AT 34.0-34.6M."	NO METALLIC SULPHIDES NOTED.	
MODD03	34.60	36.15	1.55	"PALE CREAM-GREEN MARBLE/CALC SILICATE SKARN. NON-MAGNETIC WITH MODERATE
1CM WHITE AND PINK STOCKWORK VEINING.
PINK VEINS HAVE FINE SUGARY TEXTURE AND ARE QUARTZ RICH.  WHITE VEINS
(EVIDENT AT 35.5M) HAVE MAGNETITE-RICH SELVEDGES AND POSSIBLE FINE SULPHIDE.
OCCASIONAL THREAD-LIKE RED HEMATITE VEINLETS AND HEMATITE ON
FRACTURE SURFACES."	TRACE POSSIBLE FINE SILVER SULPHIDE ?BISMUTHENITE IN WHITE VEINS.	
MODD03	36.15	38.40	2.25	"WRIGGLITE. FINELY BANDED 0.5-1MM. MODERATE CHLORITE ALTERATION. PATCHES
TO 10CM OF CALC-SILICATE STOCKWORK OF UNMINERALISED QUARTZ VEINING 
(PINKISH) 1CM AND WHITISH QUARTZ, ?ADULARIA, MAGNETITE THREAD TO 1CM
SCATTERED 0.5MM HEMATITE VEINS.
DENSE, HIGHLY MAGNETIC CORE."	"MAGNETITE 30-40%, FLUORITE ~40-50% IN BANDING."	
MODD03	38.40	39.00	0.60	"MARBLE. UNMINERALISED PALE CREAM-GREEN VERY HARD CALC-SILICATE OR MARBLE
"		
MODD03	39.00	55.80	16.80	"WRIGGLITE . FINELY BANDED AS ABOVE.
MODERATELY TO STRONGLY VEINED WITH PINK QUARTZ STOCKWORK MM TO 2CM.
WEAK CARBONATE VEINING 0.5CM.
WEAK HEMATITE VEINING.
SPOTTING WITH PALE GREEN POSSIBLE EPIDOTE AT 47.5M DENSE, HIGHLY
MAGNETIC CORE."	"DISSEMINATED FINE SULPHIDE ON FRACTURE SURFACES AT 39.1 M, OTHERWISE TRACE. TRACE FINE GRAINED PYRITE."	"PATCHY EPIDOTE SPOTTING, MODERATE CHLORITE THROUGHOUT."
MODD03	55.80	78.80	23.00	"WRIGGLITE. BANDING WITH INCREASED THICKNESS OF UP TO 0.5CM MAGNETITE/FLUORSPAR
PATCHES OF CALC-SILICATE UP TO 10CM.
QUARTZ VEINING WEAK TO MODERATE TO 1CM AS ABOVE. SOME WITH MAGNETITE IN VEIN CORES.
DENSE, HIGHLY MAGNETIC CORE.
~64.8M GREEN PYROXENE IN 1CM VEIN AND INTERGROWN WITH WRIGGLITE FLOURITE
EASILY IDENTIFABLE IN VEIN AT 67.3M.  1% DISSEMINATED FINE GRAINED PYRITE/PYRRHOTITE
AT AROUND 68M.
FROM 70M TO 78.8M: MAGNETITE.  WRIGGLITE IS IN 1-5CM ""BEDS"" AND IS INTERLAMINATED WITH CREAMY GRANULAR CALC-SILICATE OR ?FLOURITE (MEDIUM HARDNESS). ABUNDANT MUSCOVITE IN VEIN AT 71.4M.

"	MAGNETITE CONTENT 20-30%?. MOLYBDENITE CLOTS ASSOCIATED WITH QUARTZ-FLOURITE VEIN AT 65M. TRACE-1% PY THROUGHOUT. WRIGGLITE CONTENT 30-50%.	
MODD03	78.80	80.60	1.80	"SKARN. WRIGGLITE POOR.  CREAM-GREEN CALC-SILICATE AND <5% MAGNETITE.
CONTAINS SEVERAL 1-5CM QUARTZ-FELDSPAR VEINS WITH MUSCOVITE AND MOLYBDENITE
~2% IN VEIN SELVEDGES."	TRACE MOLYBDENITE APPEARING IN 1-2CM ?FLUORITE VEINS.	
MODD03	80.60	87.50	6.90	"PATCHY TO BLOTCHY MIXED MAGNETITE WRIGGLITE DOMINANT MATERIAL.
INTERLAMINATED WITH GRANULAR TEXTURED CREAM ?FLOURITE OR PYROXENE/ 
CALC-SILICATE AND OLIVE SILICEOUS CHERTY BANDS.
±MOLYBDENITE, MUSCOVITE, PYRITE (FINE-GRAINED, EPIDOTE, FLUORITE IN REDDISH-ORANGE
QUARTZ-FELDSPAR-FLUORITE VEINS MM-2CM CARBONATE VEINS, PINKISH TO WHITE,
MM TO 0.5CM."	WRIGGLITE 30-40%. TRACE TO 3% MOLYBDENITE IN VEINS (VEIN CONTENT).	
MODD03	87.50	104.70	17.20	"INCREASINGLY MAGNETITE-POOR SKARN. PATCHY MAGNETITE CLOTS AND DISJOINTED
LAMELLAE 10% IN DOMINANT GRANULAR GREENISH-CREAM MATRIX.
>92M TRENDING TO FINE GRAINED GLASSY SILICEOUS SKARN.  CREAM-GREEN TO 
GREY WITH ABUNDANT FIBROUS MAGNETITE-HEMATITE-CARBONATE VEIN NETWORKS.
REGULAR VEINS TO 4CM OF CARBONATE ?ZEOLITE/QUARTZ-FLOURITE WITH MAGNETITE-RICH SELVEDGES AND TRACE MOLYBDENITE-EPIDOTE CLOTS. ?MUSCOVITE OR TREMOLITE 5MM VEINING AT 102 AND 102.6. OCCASIONAL FINE GRANULAR QUARTZITE TEXTURE: PROTOLITH
MAY BE MOINA SST/SILTSTONE."	"UP TO 15% FINE GRAINED PYRITE CONTENT IN VEINS (VEIN CONTENT), TRACE PYRRHOTITE. <3% MAGNETITE VARIABLE. TRACE MOLYBDENITE IN VEINS."	
MODD03	104.70	105.00	0.30	"MOLYBDENITE-BEARING HEALED HYDRAULIC FAULT BRECCIA.
HIGHLY ANGULAR CLASTS OF SILTSTONE/SANDSTONE. SKARN SUPPORTED IN A PINKISH
CARBONATE MATRIX. MOLYBDENITE FLECKED ON FRACTURE SURFACES."		
MODD03	105.00	120.50	15.50	"INTERBEDDED ALTERED SANDSTONE AND SILTSTONE-MOINA SANDSTONE .
STRONGLY SILICIFIED MOTTLED GREEN-GREY TO BUFF-BROWN INTERBEDDED 
SANDSTONE AND SILTSTONE."		
MODD03	105.20	110.00	4.80	"FAULT ZONE, BROKEN GROUND 106.2-108.13 M. MODERATE QUARTZ-PYROXENE/CHLORITE, MAGNETITE ALTERED.
WEAK TO MODERATE WHITE QUARTZ-CARBONATE VEINING, MOSTLY SUB 1CM
ABUNDANT THREAD TO MM NETWORK VEINING, MAGNETITE-RICH
QUARTZ-FELDSPAR VEINING MM-CM WITH DARK MAGNETITE-RICH SELVEDGES
CARBONATE VEINING LATE."		
MODD04	0.00	4.60	4.60	"WEATHERED BASALTIC PROFILE, COLLUVIUM. TARGET: VERTICAL HOLE TO TEST WRIGGLITE SKARN
PROFILE PQ CORE. "		
MODD04	0.00	0.50	0.50	"BASALTIC SOIL, COLLUVIUM, QUARTZ PEBBLES FROM TRACK AND MINE TAILS."		
MODD04	0.50	1.70	1.20	"DEEPLY WEATHERED ORANGE-BROWN BASALTIC ROCK MN OXIDES, FE OXIDES, CLAYS, RUBBLE."		
MODD04	1.70	4.60	2.90	"MODERATELY WEATHERED ORANGE-BROWN BRECCIATED BASALTIC ROCK.
RELATIVELY FRESH BASALT CLASTS-ANGULAR IN MOTTLED ORANGE-YELLOW-BROWN
MATRIX RICH IN CLAYS AND OXIDES."		
MODD04	4.60	19.90	15.30	"AUTOBRECCIATED BASALT FLOW.  WEAKLY WEATHERED.  ANGULAR TO SUB-ROUNDED
BASALT CLASTS TO 30CM SUPPORTED IN PROBABLE GLASS AND ASH-RICH MATRIX.
CREAM-WHITE SOFT ZEOLITE THROUGHOUT. VESICULAR AT BASAL 30CM."		
MODD04	19.90	20.20	0.30	"BLACK SILT. POORLY SORTED, FLAT LYING CLEAVAGE, CONTAINS SUB-MM ANGULAR 
FRAGMENTS => VOLCANIC ASH."		
MODD04	20.20	21.30	1.10	"SAND. CREAM-WHITE FINE SAND TO SILT, QUARTZ, ?TOPAZ-RICH,  UNCONSOLIDATED. CONTAINS ~1% SUB-MM DARK SOOTY MATERIAL. GRAINS NOT  ROUNDED, MANY BLACKY GRAINS AND APPARENT SHARDS => POSSIBLE VOLCANOGENIC SAND? SHARP CONTACTS."		
MODD04	20.20	24.30	4.10	"UPWARD GRADED BROWN-BLACK VOLCANICLASTIC . CONTAINS POORLY-SORTED FRAGMENTS OF GREY-WHITE QUARTZITE CLASTS UP TO 5CM, SOME VESICULAR OR HONEYCOMB WEATHERED.  BEDDED OVER 1-30CM, SOME CONVOLUTE BEDS, ?SLUMPED.  MATRIX-SUPPORTED. MATRIX IS
BROWN-BLACK SILT WITH 1-2% FINE DISSEMINATED SULPHIDE.
OCCASIONAL PYRITIC CLOTS/CLASTS SUB-CM. SHARP CONTACTS."	1-2% FINE BRASSY SULPHIDE.	
MODD04	24.30	29.40	5.10	"POORLY SORTED ASH-DOMINANT BEDDED VOLCANICLASTIC AS ABOVE. CREAM-BROWN
WITH SCATTERED ANGULAR TO SUB-ROUND CLASTS OF QUARTZITE AND POSSIBLE 
WEATHERED WRIGGLITE (FE-RICH), SHARP UPPER CONTACT"	FINE PYRICTIC. 5% SULHIDE NOTED OVER 10CM AT 28.7 M AS CLOTS/CLASTS IN BLACK ASH BED.	
MODD04	29.40	30.00	0.60	WHITE ?QUARTZ/TOPAZ CRYSTAL SANDSTONE. BLOCKY CRYSTALS TO 1MM.		
MODD04	30.00	31.40	1.40	"BLACK ASH. ABUNDANT QUARTZITE PEBBLES HAVE PROBABLY FALLEN IN FROM ABOVE.
SHARP CONTACT AT BASE WITH WEATHERED WRIGGLITE."	TRACE FINE BRASSY SULPHIDE <0.5M.	
MODD04	31.40	36.50	5.10	"WEATHERED WRIGGLITE. INTENSE HEMATITE-LIMONITE ALTERATION TO 33.9M. INTENSE CHLORITE-LIMONITE-KAOLINITE AND GREENISH ZEOLITE.
ALT TO 36.5 VEINS ALTERED TO KAOLINITE AND GREENISH ZEOLITE."		
MODD04	36.50	43.00	3.50	"FRESH, MASSIVE WRIGGLITE SKARN. ?1MM CONVOLUTED GREEN-BLACK MAGNETITE-FLOURITE-CHLORITE SKARN.
1MM FE OXIDE COATING ON SOME JOINT SURFACES. PINK ZEOLITE COATING ON SOME JOINT SURFACES. 5CM BRITTLE FAULT AT 40.6M. WEAK  <1MM VEINS OF KAOLIN-RICH MATERIAL."	TRACE PYRITE/PYRRHOTITE COATINGS ON JOINT SURFACES.	
MODD04	43.00	51.90	8.90	"MIXED CALC-SILICATE AND WRIGGLITE SKARN. 40% WRIGGLITE AS ABOVE, 60% GREEN-WHITE-YELLOW-CREAM CALC-SILICITE.
30% CREAM-WHITE SKARN HAS FINE MM STOCKWORK OF PALE GREEN SILICATE
VEINING. ROCK IS FINELY GRANULAR ?RELICT SANDSTONE. VERY HARD, VERY SILICEOUS.
30% YELLOW-CREAM SKARN HAS SUGARY TEXTURE AND V. HARD. SOME CREAM-YELLOW
SUB MM GARNETS VISIBLE.  VERY HARD =>PROBABLE GARNET-RICH SKARN."	MAGNETITE WRIGGLITE AND TRACE PYRITE AND PYRRHOTITE.	
MODD04	51.90	74.70	22.80	"MASSIVE WRIGGLITE SKARN. WRIGGLITE AS AT 36.5M
FINELY SPOTTED WITH ?GARNET ALTERATION FROM 51.9 TO  55.3M.
PATCH OF SUB-MM EPIDOTE ALTERATION OVER 30CM AT 55M.
WEAK CM SCALE VEINING WITH PINK QUARTZITE.  10CM PATCH OF SEMI-MASSIVE 
MAGNETITE AT 55.5M. HARD TO DRILL, GARNET VISIBLE ON FRACTURE AT 55.3M."	"TRACE PYRITE ±PYRRHOTITE, MARCASITE THROUGHOUT."	MODERATE CHLORITE-GARNET-EPIDOTE.
MODD04	67.80	69.10	1.30	"STRONG STOCKWORK OF CREAM QUARTZ-FLOURITE/FELDPSAR VEINING TO 3CM.
MINOR FAULT/SHEAR OVER 5CM. UP TO 20% INTERMIXED CALC-SILICATE FROM 66M."		
MODD04	74.70	83.00	8.30	"20% WRIGGLITE, 80%, CALC-CILICATE SKARN."	 	
MODD04	74.70	83.00	8.30	"CREAM, PALE GREEN AND PINK-CREAM MOTTLED SKARN WITH SPOTTY TO 
COLLIFORM-LIKE PATCHES OF PINK-CREAM GARNET ALTERATION.
COMPLEX VEINING WITH MODERATE INTENSITY THREAD-LIKE ANNEALED DARK
STOCKWORK AND CM SCALE QUARTZ-FLOURITE±WOLFRAMITE AND MOLYBDENITE VEINS WITH SUB-CM FINE MAGNETIC SELVEDGES. WRIGGLITE PATCHY AND DISJOINTED.  2OCM PATCH OF SEMI-MASSIVE MOLYBDENITE AT 79.1M.  TRANSITIONAL DOWNHOLE BOUNDARY OVER 5CM."	"TRACE MOLYBDENITE AND WOLFRAMITE IN SILICATE VEINS. WOLFRAM IN 2CM VEIN AT 75.1M, LOCALLY 2%. DISSEMINATED 1-2MM PYRITE BLEBS OVER 20CM AT 80.8M."	MODERATE RED GARNET AMD CHLORITE.
MODD04	83.00	88.60	5.60	"PINKISH CREAM GARNET-RICH CALC-SILICATE SKARN. VERY HARD MOTTLED AND SPOTTED WITH WEAK BLACK MAGNETITE AND PALE GREEN EPIDOTE PYROXENE ALTERATION.
WEAK VEINING WITH QUARTZ-FELDSPAR-FLOURITE AND MAGNETITE SELVEDGES MM TO CM
SCALE AS ABOVE. TRANSITIONAL DOWNHOLE BOUNDARY OVER 30CM."	"TRACE WOLFRAM IN VEIN CORES, TRACE PYRITE."	STRONG GARNET. WEAK EPIDOTE-PYROXENE.
MODD04	88.60	90.80	2.20	"MIXED CREAM AND PALE GREEN AND BLACK CALC-SILICATE-GARNET-MAGNETITE 
SKARN, VERY HARD WITH PATCHY VEIN RELATED MAGNETITE MINERALISATION.  10-15%
PATCHY VEIN RELATED FINE GRAINED PYRITE 3%.
INTENSE MAGNETITE DOMINANT STOCKWORK VEINING DOMINANTLY SUB-CM MODERATE MM-0.5CM PINK-WHITE QUARTZ-FLOURITE VEINING±MOLYBDENITE AND WOLFRAMITE."	2% PYRITE. TRACE MOLYBDENITE AND WOLFRAMITE IN SILICATE VEINS.	
MODD04	90.80	101.20	10.40	"ALTERED MOINA SANDSTONE.  CREAM-BROWN TO GREY-GREEN FINE GRAINED 
MODERATELY QUARTZ-CHLORITE ALTERED SANDSTONE AND SILTSTONE.
STRONGLY BROKEN CORE WITH INTERSECTING FRACTURES ACUTE TO VCAS
40-40° TO VCA. FROM 97.5-97.7M: 20CM INTENSELY SHEARED PUGGY FAULT ZONE AT 97.5M WITH STRONG-INTENSE GREEN-WHITE CLAY AND PINK ZEOLITE ALTERATION. FAULT 70 DEGREES TO VCA.
STRONG EUHEDRAL ± 1MM PYRITE ALTERATION IN 0.5CM VEINS FROM LOCAL TO 
FAULT.  LOCALLY 60% PY IN VEINS. PATCHY, STRONG VEINING WITH THREAD-LIKE TO SUB-CM.
PINK-RED ZEOLITE, QUARTZ-ZEOLITE, QUARTZ-FELDSPAR FLOURITE± WOLFRAMITE. GENERALLY 40 TO 80 DEGREES TO VCA."	MODERATE PYRITE LOCALISED AROUND FAULT. TRACE WOLFRAMITE-VEIN RELATED. 	WEAK MAGNETITE. 1MM TALC-KAOLINITE COATINGS ON FRACTURE SURFACES.
						
						
						
						
						
						
						
