The Tx loop vertices in the Outer-Rim field data and field report are wrong for Tx Loop 2.

The vertices for Tx Loop 2 didn't go all the way around the outside of Loop 1
(eg. not as shown in the Outer-Rim report Figure 3) but rather the two loops shared one common side.

If you look at Outer-Rim report Figure 1 and interpret the red lines as two separate polygons
then L1 is the SW loop and L2 is the NE loop.

In other words L1 and L2 are roughly the same area as each other; L2 is not roughly twice the area of L1.

...Phil Muir
...21/5/2013
