SCINTREX IPR-12 Gradient array and dipole-dipole IP data

Acquired by SCINTREX Pty Ltd for RGC in 1996 over the Gowrie Park Grid

Receiver: IPR12

Transmitter: TSQ-3 3000kW

Gradient array potential dipole: 25m

Current electrode separation: typically 2km

Dipole Dipole Line: 3600

Dipole length: 50m



Total of four gradient arrays surveyed gowpk1.lst to gowpk4.lst are the RAW listing files

gp_ip.xls EXCEL spreadsheet of data

3600 files contain dipole-dipole data 