These data files have been compressed with the PKZIP packing utility 
program.  The program PKZ204G.EXE has been included with this data set 
on diskette 1.

Typing "PKUNZIP filename.ZIP" unpacks a *.ZIP file.  PKUNZIP is self-
documenting if you type "PKUNZIP".

This data is reprocessed from Zonge jobs 864 (1988) and 968 
(1990), Basin Lake, Tasmania.
Data is archived on a line by line basis.  Only averaged data 
are included for each line.  

I file:  old Zonge precursor to mde file.
AD file:  old averaged data format.
AVG file:  modern file format for averaged data.
MDE file:  modern file that controls data processing flow.
ZCR file:  Zonge file of Cagniard resistivity and impedance 
           phase.
ZSR file:  Zonge file of Static corrected resistivity and 
           impedance phase.
XCR, XPZ and XSR:  HP format plot files.  Can be imported into 
           Coreldraw.

Zonge Engineering & Research Organization


